SunOS 5.5 Maintenance Commands sysdef (1M )

NAME sysdef − output system definition

SYNOPSIS /usr/sbin/sysdef [ − n namelist ]

/usr/sbin/sysdef [ − h ] [ − d ]

AVAILABILITY SUNWcsu

DESCRIPTION sysdef outputs the current system definition in tabular form. It lists all hardware devices, as well as pseudo devices, system devices, loadable modules, and the values of selected kernel tunable parameters.

It generates the output by analyzing the named bootable operating system file (namelist) and extracting the configuration information from it.

The default system namelist is /dev/kmem .

OPTIONS − n namelist Specifies a namelist other than the default (/dev/kmem ). The namelist specified must be a valid bootable operating system.

− h Prints the identifier of the current host in hexadecimal. This numeric value is unique across all Sun hosts.

− d The output includes the configuration of system peripherals formatted as a device tree.

EXAMPLES The following example displays the format of the sysdef − d output:

example% sysdef − d

Node ’Sun 4/60’, unit #0 (no driver)

Node ’options’, unit #0 (no driver)

Node ’zs’, unit #0

Node ’zs’, unit #1

Node ’fd’, unit #0

Node ’audio’, unit #0

Node ’sbus’, unit #0

Node ’dma’, unit #0

Node ’esp’, unit #0

Node ’st’, unit #1 (no driver)

Node ’st’, unit #0

Node ’sd’, unit #2

Node ’sd’, unit #1

Node ’sd’, unit #0

Node ’le’, unit #0

Node ’bwtwo’, unit #0

Node ’auxiliary-io’, unit #0

Node ’interrupt-enable’, unit #0

Node ’memory-error’, unit #0

Node ’counter-timer’, unit #0

Node ’eeprom’, unit #0 modified 10 Sep 1994 1M-653 sysdef (1M ) Maintenance Commands SunOS 5.5

FILES /dev/kmem default operating system image

SEE ALSO hostid (1), prtconf (1M), nlist (3E)

1M-654 modified 10 Sep 1994