SunOS 5.5 Maintenance Commands syslogd (1M )

NAME syslogd − log system messages

SYNOPSIS /usr/sbin/syslogd [ − d ] [ − f configfile] [ − m markinterval ] [ − p path ]

AVAILABILITY SUNWcsu

DESCRIPTION syslogd reads and forwards system messages to the appropriate log files and/or users, depending upon the priority of a message and the system facility from which it originates. The configuration file /etc/syslog.conf (see syslog.conf (4)) controls where messages are forwarded. syslogd logs a mark (timestamp) message every markinterval minutes (default 20) at priority LOG_INFO to the facility whose name is given as mark in the syslog.conf file.

A system message consists of a single line of text, which may be prefixed with a priority code number enclosed in angle-brackets (<>); priorities are defined in <sys/syslog.h> .

syslogd reads from the STREAMS log driver, /dev/log , and from any transport provider specified in /etc/netconfig , /etc/net/transport/hosts , and /etc/net/transport/services .

syslogd reads the configuration file when it starts up, and again whenever it receives a

HUP signal (see signal (5), at which time it also closes all files it has open, re-reads its configuration file, and then opens only the log files that are listed in that file. syslogd exits when it receives a TERM signal.

As it starts up, syslogd creates the file /etc/syslog.pid , if possible, containing its process identifier (PID).

OPTIONS − d Turn on debugging.

− f configfile Specify an alternate configuration file.

− m markinterval Specify an interval, in minutes, between mark messages.

− p path Specify an alternative log device name. The default is /dev/log .

FILES /etc/syslog.conf configuration file

/etc/syslog.pid process ID

/dev/log STREAMS log driver

/etc/netconfig specifies the transport providers available on the system

/etc/net/transport/hosts network hosts for each transport

/etc/net/transport/services network services for each transport

SEE ALSO logger (1), syslog (3), syslog.conf (4), signal (5), log(7D) modified 03 Aug 1994 1M-659