SunOS 5.5 Maintenance Commands sysidconfig (1M )

NAME sysidconfig − execute system configuration applications, or define set of system configuration applications

SYNOPSIS sysidconfig [ − b basedir ] [ − l ] [ − a application ] [ − r application ] [ − v ]

AVAILABILITY SUNWadmap

DESCRIPTION Invoked without any options, the sysidconfig program executes a list of applications. An application on this list is referred to as a "system configuration application." Every application on this list will be passed one command-line argument, − c. This flag will cause the system configuration application to perform its configuration function. Without options, sysidconfig should only be invoked by startup scripts, which occurs during the initial installation and during a reconfigure reboot.

All applications on the list will be executed, if possible. All activity taken by the sysidconfig program is logged in the sysidconfig log file, /var/log/sysidconfig.log . If one or more of the applications on the list are either not present at execution time, are not executable, or execute but return a failure code upon completion, then that information will be logged as well. Successful completion of the program can be assumed if no error message is present in the log file. Programs are executed sequentially, with only one configuration application active at a time.

Executed with the − l, − a, or − r options, the sysidconfig program allows the superuser to list the defined configuration applications, and to add items to or remove items from that list. Running sysidconfig with options is the only way to view or manipulate the list.

Only the superuser can execute the sysidconfig program with options.

The − b and -v options change the behavior of sysidconfig , and can be used with or without the list manipulation options discussed above. The − b basedir option is used to specify a reference root directory other than the default, /. The − v option duplicates the log file output on stdout .

By default, no SPARC applications exist on this list. However, the x86 system is delivered with one application, kdmconfig (1M), on the list. kdmconfig is an x86-specific program that is not delivered on SPARC systems.

This application is an extension of the sysidtool (1M) suite of programs. It is executed during initial installation and during a reconfigure reboot, before the window system has been started. Graphical User Interface (GUI) applications will not execute successfully if they are added to the list of configuration applications via sysidconfig − a.

This program is referenced, but not fully described, in the sysidtool (1M) manual page.

OPTIONS The valid options are:

− b basedir Specify an alternate base directory (/ is defined as the default base directory if no other is specified). The specified directory is used as the root directory when adding, listing, removing, or executing configuration applications. The log file where information is recorded is in /var/log , relative to the specified basedir. In the log file, the basedir is not noted.

modified 8 December 1993 1M-655 sysidconfig (1M ) Maintenance Commands SunOS 5.5

This means, for example, that if the superuser on a diskless client’s server executes:

sysidconfig − b /export/root/ client − a /sbin/ someapp then the diskless client client would have /sbin/ someappexecuted upon reconfigure reboot. The diskless client’s log file would note that

/sbin/ someappwas added, not /export/root/client/sbin/ someapp.

− l List defined configuration applications. Applications will be executed one at a time, in the order shown in the list.

− a application Add the named application to the list of defined applications. When next invoked without arguments, sysidconfig will run this newly added application after all previously defined applications. application must be a fully qualified path name that is not currently on the list of applications to execute.

− r application Remove the named application from the list of defined applications.

application must be a fully qualified path name and it must be on the existing list of applications to execute.

− v Verbose mode. This option echoes all information sent to the log file to stdout . Such information includes timestamp information about when the program was executed, the names of applications being executed, and results of those executions.

RETURN VALUES The sysidconfig program will return 0 if it completes successfully.

When executed with the − r or − a options, error conditions or warnings will be reported on stderr . If the requested action completes successfully, an exit code of 0 will be returned.

ERRORS EPERM The program was executed by a user other than the superuser.

EINVAL Option − l, − a, or − r was passed and the action could not be completed successfully.

FILES /var/log/sysidconfig.log

SEE ALSO sys-unconfig (1M), sysidtool (1M) x86 Only kdmconfig (1M)

DIAGNOSTICS When run without options, a log of the sysidconfig program’s activity can be found in

/var/log/sysidconfig.log . This file contains a timestamp log of each program executed, its resulting stderr output, and its exit code. If an application in the list was not found or is not executable, that will also be noted.

1M-656 modified 8 December 1993