cgsix (7D ) Devices SunOS 5.5

NAME cgsix − accelerated 8-bit color frame buffer

SYNOPSIS /dev/fbs/cgsix n

DESCRIPTION cgsix is a low-end graphics accelerator designed to enhance vector and polygon drawing performance. It has an 8-bit color frame buffer and provides the standard frame buffer interface as defined in fbio (7I).

In addition, cgsix supports the following cgsix-specific IOCTL, defined in <sys/fbio.h> .

FBIOGXINFO Returns cgsix-specific information about the hardware. See the definition of cg6_info in <sys/fbio.h> for more information.

cgsix has registers and memory that may be mapped with mmap (2), using the offsets defined in <sys/cg6reg.h> .

FILES /dev/fbs/cgsix0

SEE ALSO mmap (2), fbio (7I)

7D-64 modified 27 Mar 1992