SunOS 5.5 Devices pcram (7D )

NAME pcram − PCMCIA RAM memory card device driver

SYNOPSIS pcmem@ <socket>/pcram@<technology>,0:c pcmem@ <socket>/pcram@<technology>,0:c,raw

DESCRIPTION The PCMCIA RAM memory card device driver supports disk-like I/O access to any standard PCMCIA static random access memory (SRAM) card and dynamic random access memory (DRAM) card. The driver supports standard PCMCIA SRAM/DRAM cards that contain a Card Information Structure (CIS). RAM card densities in the 512Kilobytes to

64Mbyte range are supported.

FILES /kernel/drv/pcram pcram driver

/dev/dsk/c ntndnsn block files

/dev/rdsk/c ntndnsn raw files where:

cn controller n tn technology type n

0x1 ROM, 0x2 OTPROM, 0x3 EPROM,

0x4 EEPROM, 0x5 FLASH, 0x6 SRAM,

0x7 DRAM dn technology region in type n sn slice n

SEE ALSO fdformat (1), pcmcia (4), dkio (7I), pcmem (7D) modified 20 Mar 1995 7D-249