tpf (7D ) Devices SunOS 5.5

NAME tpf − Platform Specific Module (PSM) for Tricord Systems Enterprise Server Models

ES3000, ES4000 and ES5000.

AVAILABILITY x86

DESCRIPTION tpf provides the platform dependent functions for Solaris X86MP support. These functions adhere to the PSMI Specifications. (Platform Specific Module Interface

Specifications.) Tricord Systems Enterprise Servers are Intel APIC based MP platforms which run from 1 to 12 Intel processors. The tpf psm supports dynamic interrupt distribution across all processors in an MP configuration.

The psm is automatically invoked on an ESxxxx platform at system boot time.

FILES /kernel/mach/tpf

MP module.

7D-378 modified 23 Jan 1995