SunOS 5.5 Kernel Functions for Drivers uwritec (9F)

NAME uwritec − remove a character from a uio structure

SYNOPSIS #include <sys/uio.h> int uwritec (uio_t ∗uio_p);

INTERFACE

LEVEL Architecture independent level 1 (DDI/DKI).

ARGUMENTS uio_p Pointer to the uio(9S) structure.

DESCRIPTION uwritec( ) returns a character from the uio structure pointed to by uio_p, and updates the uio structure as for uiomove (9F).

RETURN VALUES The next character for processing is returned on success, and -1 is returned if uio is empty or there is an error.

CONTEXT uwritec( ) can be called from user or interrupt context.

SEE ALSO uiomove (9F), ureadc (9F), iovec (9S), uio(9S)

WritingDevice Drivers modified 11 Apr 1991 9F-391