dev_ops (9S) Data Structures for Drivers SunOS 5.5

NAME dev_ops − device operations structure

SYNOPSIS #include <sys/conf.h>

#include <sys/devops.h>

INTERFACE

LEVEL Solaris DDI specific (Solaris DDI).

DESCRIPTION dev_ops contains driver common fields and pointers to the bus_ops and/or cb_ops (9S).

Following are the device functions provided in the device operations structure. All fields must be set at compile time.

devo_rev Driver build version. Set this to DEVO_REV.

devo_refcnt Driver reference count. Set this to 0.

devo_getinfo Get device driver information (see getinfo (9E)).

devo_identify Determine if a driver is associated with a device (see identify (9E)).

devo_probe Probe device (see probe (9E)).

devo_attach Attach driver to dev_info (see attach (9E)).

devo_detach Detach/prepare driver to unload (see detach (9E)).

devo_reset Reset device (Not supported in this release).

devo_cb_ops Pointer to cb_ops (9S) structure for leaf drivers.

devo_bus_ops Pointer to bus operations structure for nexus drivers. Set this to

NULL if this is for a leaf driver.

STRUCTURE

MEMBERS int devo_rev;

int devo_refcnt;

int (∗devo_getinfo)(dev_info_t ∗dip, ddi_info_cmd_t infocmd, void ∗arg, void ∗∗result);

int (∗devo_identify)(dev_info_t ∗dip);

int (∗devo_probe)(dev_info_t ∗dip);

int (∗devo_attach)(dev_info_t ∗dip, ddi_attach_cmd_t cmd);

int (∗devo_detach)(dev_info_t ∗dip, ddi_detach_cmd_t cmd);

int (∗devo_reset)(dev_info_t ∗dip, ddi_reset_cmd_t cmd);

struct cb_ops ∗devo_cb_ops;

struct bus_ops ∗devo_bus_ops;

SEE ALSO attach (9E), detach (9E), getinfo (9E), identify (9E), probe (9E)

WritingDevice Drivers

9S-40 modified 18 Jul 1994