SunOS 5.5 Data Structures for Drivers modldrv (9S)

NAME modldrv − linkage structure for loadable drivers

SYNOPSIS #include <sys/modctl.h>

INTERFACE

LEVEL Solaris DDI specific (Solaris DDI)

DESCRIPTION The modldrv structure is used by device drivers to export driver specific information to the kernel.

STRUCTURE

MEMBERS struct mod_ops ∗drv_modops;

char ∗drv_linkinfo;

struct dev_ops ∗drv_dev_ops;

drv_modops Must always be initialized to the address of mod_driverops . This identifies the module as a loadable driver.

drv_linkinfo Can be any string up to MODMAXNAMELEN, and is used to describe the module. This is usually the name of the driver, but can contain other information (such as a version number).

drv_dev_ops Pointer to the driver’s dev_ops (9S) structure.

SEE ALSO add_drv (1M), dev_ops (9S), modlinkage(9S)

WritingDevice Drivers modified 7 Jun 1993 9S-51