modlinkage (9S) Data Structures for Drivers SunOS 5.5

NAME modlinkage − module linkage structure

SYNOPSIS #include <sys/modctl.h>

INTERFACE

LEVEL Solaris DDI specific (Solaris DDI)

DESCRIPTION The modlinkage structure is provided by the module writer to the routines which install, remove, and retrieve information from a module. See _init (9E), _fini (9E), and _info (9E).

ml_rev Is the revision of the loadable modules system. This must have the value MODREV_1.

ml_linkage Is a null terminated array of pointers to linkage structures. For driver modules there is only one linkage structure.

STRUCTURE

MEMBERS int ml_rev void ∗ml_linkage[4];

SEE ALSO add_drv (1M), _fini (9E), _info (9E), _init (9E), modldrv (9S), modlstrmod (9S)

WritingDevice Drivers

9S-52 modified 18 Sep 1992