module_info (9S) Data Structures for Drivers SunOS 5.5

NAME module_info − STREAMS driver identification and limit value structure

SYNOPSIS #include <sys/stream.h>

INTERFACE

LEVEL Architecture independent level 1 (DDI/DKI).

DESCRIPTION When a module or driver is declared, several identification and limit values can be set.

These values are stored in the module_info structure.

The module_info structure is intended to be read-only. However, the flow control limits

(mi_hiwat and mi_lowat ) and the packet size limits (mi_minpsz and mi_maxpsz ) are copied to the QUEUE structure, where they may be modified.

STRUCTURE

MEMBERS ushort mi_idnum; /∗ module ID number ∗/ char ∗mi_idname; /∗ module name ∗/ long mi_minpsz; /∗ minimum packet size ∗/ long mi_maxpsz; /∗ maximum packet size ∗/ ulong mi_hiwat; /∗ high water mark ∗/ ulong mi_lowat; /∗ low water mark ∗/

The constant FMNAMESZ , limiting the length of a module’s name, is set to eight in this release.

SEE ALSO queue (9S)

STREAMSProgramming Guide

9S-54 modified 11 Apr 1991