SunOS 5.5 Data Structures for Drivers copyreq (9S)

NAME copyreq − STREAMS data structure for the M_COPYIN and the M_COPYOUT message types

SYNOPSIS #include <sys/stream.h>

INTERFACE

LEVEL Architecture independent level 1 (DDI/DKI).

DESCRIPTION The data structure for the M_COPYIN and the M_COPYOUT message types.

STRUCTURE

MEMBERS int cq_cmd; / ∗ ioctl command (from ioc_cmd) ∗/ cred_t ∗cq_cr; / ∗ full credentials ∗/ uint cq_id; / ∗ ioctl id (from ioc_id) ∗/ caddr_t cq_addr; / ∗ address to copy data to/from ∗/ uint cq_size; / ∗ number of bytes to copy ∗/ int cq_flag; / ∗ see below ∗/ mblk_t ∗cq_private; / ∗ private state information ∗/ long cq_filler[4]; / ∗ reserved for future use ∗/

/ ∗ cq_flag values ∗/

#define STRCANON 0x01 / ∗ b_cont data block contains ∗/

/ ∗ canonical format specifier ∗/

#define RECOPY 0x02 / ∗ perform I_STR copyin again, ∗/

/ ∗ this time using canonical ∗/

/ ∗ format specifier ∗/

SEE ALSO STREAMSProgramming Guide modified 7 Mar 1994 9S-15