PEXEscapeWithReply (3) Solaris PEXlib Reference Manual

NAME PEXEscapeWithReply - PEX Escape With Reply

SYNTAX char ∗PEXEscapeWithReply (Display ∗display, unsigned long escape_id, int length, char

∗escape_data , unsigned long ∗reply_length_return)

PARAMETERS display A pointer to a display structure returned by a successful XOpenDisplay call.

escape_id The escape identifier.

length The length, in bytes, of data for the escape request.

escape_data A pointer to data for the escape request.

reply_length_return

Returns the length, in bytes, of the reply data.

RETURNS A pointer to the escape reply data; a null pointer if unsuccessful.

DESCRIPTION PEXEscapeWithReply has an implementation-dependent effect. It is similar to PEXEscape (3) except it has return data. It is provided as a way for implementation-specific functionality to be accessed. The complete interface and behavior for each specified escape identifier should be specified by the individual PEX server implementation.

If the specified escape identifier is not supported, a value error is generated. The table below lists the supported escape identifiers.

The reply data is returned in memory allocated by PEXlib. XFree should be called to deallocate the memory.

Escape Identifier Description

PEXSunEscIdGetMarkerDescr Get marker descriptions

PEXSunEscIdGetExtRendAttr Get extended renderer attributes

PEXSunEscIdGetExtRendAttrDyn Get extended renderer dynamics

ES_ESCAPE_SWAPBUFFERCONTENT Inquire update action during buffer swap

ERRORS Escape-dependent

See documentation provided with the individual PEX server implementation.

BadValue

The specified escape identifier is unsupported.

SEE ALSO PEXEscape (3)

80 modified November 1995