Solaris PEXlib Reference Manual PEXSetPWAttributeMask (3)

NAME PEXSetPWAttributeMask - Macro to Setup Workstation Attributes Value Mask

SYNTAX PEXSetPWAttributeMask( mask, attr)

PARAMETERS mask The address of the value mask - an array of two unsigned long.

attr A single workstation attribute bitmask constant.

DESCRIPTION This is a utility macro to aid in setting up the bitmask for the workstation attributes.

The following constants must be used:

PEXPWBufferUpdate PEXPWInvisibilityExcl

PEXPWColorApproxTable PEXPWInvisibilityIncl

PEXPWColorTable PEXPWLightTable

PEXPWCurBufferMode PEXPWLineBundle

PEXPWCurHLHSRMode PEXPWMarkerBundle

PEXPWCurNPCSubVolume PEXPWNumPriorities

PEXPWCurViewport PEXPWPatternTable

PEXPWDefinedViews PEXPWPostedStructures

PEXPWDepthCueTable PEXPWReqBufferMode

PEXPWDisplaySurface PEXPWReqHLHSRMode

PEXPWDisplayUpdate PEXPWReqNPCSubVolume

PEXPWDrawable PEXPWReqViewport

PEXPWEdgeBundle PEXPWTextBundle

PEXPWHLHSRUpdate PEXPWTextFontTable

PEXPWHighlightExcl PEXPWViewUpdate

PEXPWHighlightIncl PEXPWVisualState

PEXPWInteriorBundle PEXPWWorkstationUpdate

Note that this macro does multiple evaluations of the value for attr.

ERRORS None

SEE ALSO PEXGetWorkstationAttributes (3) modified November 1995 349